README

This Arduino code works with the Curie TinyTile microcontroller, which receives data from the Android App.

The microcontroller commands the HERO Glove actuators to move to full extension or full retraction to provide hand extension or grip assistance.